EXTRA HELP FILES FOR XPENTOR VOODOO 3 2000-3000 DRIVERS

Driver Version: X-GAMERS 


----------------
AGP COMMAND FIFO
----------------
THIS OPTION ALLOWS YOU TO DETERMINE WHAT TYPE OF AGP YOU HAVE.
IF YOU ARE NOT SURE ABOUT YOUR AGP, CHOOSE AUTO DETECT!

-----------
VIA CHIPSET
-----------
WARNING: THIS OPTION CAN BE USED ONLY ON MOTHERBOARD WITH 
         VIA CHIPSET CONTROLLER
PERFORMANCE: SLIGHTLY IMPROVES YOUR PERFORMANCE
COMPATIBILITY: GIVES MORE STABILITY 
BIOS DEFAULTS: WORKS DEPEND ON THE BIOS SETUP
DISABLED: USED ONLY BY A MOTHERBOARD WITHOUT VIA CHIPSET CONTROLLER

---------------------
CORE CLOCK
---------------------
THIS OPTION LETS YOU DETERMINE THE TRANSFER SPEED OF YOUR MEMORY.
183 MHZ IS THE DEFAULT SPEED.
WARNING: ACCORDING TO 3DFX, VOODOO SERIES CAN NOT BE OVERCLOCKED OVER 10%!!

-------------
ANTI-ALIASING
-------------
THIS OPTION HELPS YOU TO GET RID OF THE JAGGED LINES
IT REDUCES PERFORMANCE.


------------------
GUARDBAND CLIPPING
------------------
ENABLE THIS FEATURE LEADS TO A SLIGHT IMPROVEMENT IN PERFORMANCE

----------------------
HIDDEN SURFACE REMOVAL
----------------------
THIS FEATURE IS USED FOR ELIMINATING THE UNIMPORTANT TEXTURES OR OBJECTS
SOMETIMES WHEN IT'S ENABLED MAY CAUSE A TRANSPARENT OBJECT OR INCORRECT RENDERING 
THIS WILL INCREASE THE PERFORMANCE SLIGHTLY

-------------------------------
DIRECT3D TRANSFORM AND LIGHTING
-------------------------------
ENABLE THIS FEATURE HELPS YOU TO BOOST THE DIRECT3D PERFORMANCE UP TO 30% FASTER!!

----------
VERTEX FOG
----------
THIS OPTION SHOULD BE ENABLED! VERTEX FOG WILL INCREASE THE PERFORMANCE SLIGTHLY
AND GIVES BETTER VISUAL (ESPECIALLY WHEN IT'S RENDERING SMOKES)

-------------------
SPECULAR GOURAUD
-------------------
THIS ALSO SHOULD BE ENABLED FOR BETTER PERFORMANCE AND VISUALS !

---------------
POINT SAMPLING
---------------
THIS WILL IMPROVE YOUR VISUAL QUALITY WITHOUT DECREASING THE HARDWARE PERFORMANCE!